How to use TCL files

* Copy the C++ files for your test-bench and HLS function, respectively, and also copy the *script.tcl* file into a desired folder
* Open the Vivado HLS Command Prompt and navigate to that folder
* Execute the command below to generate the HLS project.

vivado\_hls -f script.tcl

* + Execute the command below to open the generated Vivado HLS project

vivado\_hls -p <generated project name>